Single function needed for ST1.

You must not modify registers during function. By end, must be same as originally was.  
ie, you push eax, ebx ect onto stack to save (entry code), and pop on (exit code).

Return value always as eax. NOT ANY OTHER VALUES.  
-so don’t push and pop eax